<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.40.8-Bratislava">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <links/>
  <dates/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["NTF_Lambert_Zone_I",BASEGEOGCRS["NTF",DATUM["Nouvelle Triangulation Francaise",ELLIPSOID["Clarke 1880 (IGN)",6378249.2,293.46602,LENGTHUNIT["metre",1]],ID["EPSG",6275]],PRIMEM["Greenwich",0,ANGLEUNIT["Degree",0.0174532925199433]]],CONVERSION["unnamed",METHOD["Lambert Conic Conformal (2SP)",ID["EPSG",9802]],PARAMETER["Latitude of false origin",49.5,ANGLEUNIT["Degree",0.0174532925199433],ID["EPSG",8821]],PARAMETER["Longitude of false origin",2.3372291667,ANGLEUNIT["Degree",0.0174532925199433],ID["EPSG",8822]],PARAMETER["Latitude of 1st standard parallel",48.5985227778,ANGLEUNIT["Degree",0.0174532925199433],ID["EPSG",8823]],PARAMETER["Latitude of 2nd standard parallel",50.3959116667,ANGLEUNIT["Degree",0.0174532925199433],ID["EPSG",8824]],PARAMETER["Easting at false origin",600000,LENGTHUNIT["metre",1],ID["EPSG",8826]],PARAMETER["Northing at false origin",200000,LENGTHUNIT["metre",1],ID["EPSG",8827]]],CS[Cartesian,2],AXIS["(E)",east,ORDER[1],LENGTHUNIT["metre",1,ID["EPSG",9001]]],AXIS["(N)",north,ORDER[2],LENGTHUNIT["metre",1,ID["EPSG",9001]]]]</wkt>
      <proj4>+proj=lcc +lat_0=49.5 +lon_0=2.3372291667 +lat_1=48.5985227778 +lat_2=50.3959116667 +x_0=600000 +y_0=200000 +a=6378249.2 +rf=293.46602 +towgs84=-168,-60,320,0,0,0,0 +units=m +no_defs +type=crs</proj4>
      <srsid>0</srsid>
      <srid>0</srid>
      <authid></authid>
      <description>NTF_Lambert_Zone_I</description>
      <projectionacronym></projectionacronym>
      <ellipsoidacronym>PARAMETER:6378249.20000000018626451:6356514.99990419391542673</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent/>
</qgis>
